INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP. Pontiac 6000 1988

For 1990-2009 cars

# INTERMITTENT OR IN-OPERATIVE CENTER HIGH MOUNTED STOP LAMP

INTERMITTENT OR INOPERATIVE CENTER HIGH MOUNTED STOP LAMP DUE TO A HEAT DISTORTED SOCKET

#### MODELS AFFECTED 1988 SUNBIRD COUPE ---------------

If an intermittent or inoperative center high mounted stop lamp due to a heat distorted socket is encountered in a 1988 Sunbird Coupe both sockets must be installed using part number 5972532 available from GMSPO. All service stock of this part uses a new heat resistant material. The production stock was corrected beginning with VIN J7544390.

#### WARRANTY INFORMATION

Labor Operation: N1000

Labor Time : 0.2 hrs

Part Number : 5972532 (2)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.