PARK BRAKE CABLE SERVICE REINSTALL RETAINING CLIP. Pontiac 6000 1984

For 1990-2009 cars

# PARK BRAKE CABLE SERVICE REINSTALL RETAINING CLIP

1984-87 STE

The park brake cables are clipped to the rear caliper park brake lever at the factory to maintain proper cable location. When caliper or cable service is required, the retaining clips should be reinstalled.

Vehicles built between 1984 and mid 1986 were not built with retaining clips. When servicing vehicles without retaining clips, add the clips, P/N 14102324, as shown in the Illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.