2ND GEAR STARTS 125/125C TRANS MISSION CONTROL VALVE ASSEMBLY. Pontiac 6000 1982

For 1990-2009 cars

# 2ND GEAR STARTS 125/125C TRANS MISSION CONTROL VALVE ASSEMBLY

#### VEHICLES AFFECTED: 1982 - 84 Vehicles Equipped With THM 125/125-C Transmissions

Some 1982, and 1983, CE model only, and early 1984 model THM 125/125-C transmissions may exhibit a second gear start, which is best described as the transmission starting in second gear range instead of first gear range.

Starting with the serial numbers listed below a new control valve body assembly went into production to correct this second gear start condition.

When servicing any 1982 or 1983 CE model only, or early 1984 model THM 125/125-C transmission for this second gear start condition, replace the control valve body assembly with the control valve body assembly listed in the dealership parts manual.

#### MODEL SERIAL NO. MODEL SERIAL NO. ----- ---------- ----- ---------- CA 1674 EQ 6883 CB 91946 HC 1613 CE 47452 HM 1823 CF 4607 HP 1053 CT 3519 HS 8740 EB 2152 HX 3361 EF 5809 HY 13184 EI 3760 PD 2104 EJ 1006 PE 42048 EK 8183 PF 13478 EL 3594 PG 36699 EM 2528 PJ 4822 EN 4984 PW 47580 EP 1989

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.