ABS PUMP MOTOR REPLACEMENT PROCEDURE (INFORMATIONAL). Pontiac 6000 1987

For 1990-2009 cars

# ABS PUMP MOTOR REPLACEMENT PROCEDURE (INFORMATIONAL)

#### Subject: ABS PUMP MOTOR REPLACEMENT PROCEDURE (INFORMATION)

#### Models Affected: 1986-90 6000 MODELS

Some 1986-1990 6000 may experience a failed ABS pump motor. This condition may be caused by a faulty pump motor relay. The pump motor relay contacts may become welded together causing the pump motor to continue running after the specified system pressure is attained.

To correct this condition and prevent repeat failures, the appropriate pump motor relay listed below should be replaced any time a pump motor failure occurs.

MODEL 1986-1987 1988 1989-1990 ----- --------- ---- 6000 25525848 25553347 25553347

Parts are currently available from GMSPO.

For warranty purposes use Labor Operation H2475 at .2 hour.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.