INOP FOG LAMP SWITCH INSTALL NEW SWITCH BEZEL. Pontiac 6000 1984

For 1990-2009 cars

# INOP FOG LAMP SWITCH INSTALL NEW SWITCH BEZEL

#### VEHICLES AFFECTED: 1984 and 1985 6000 STE

#### CONDITION:

--------- The fog lamp switch in some 1984 or 1985 STE vehicles may be difficult to turn off or on.

#### CAUSE:

------ The condition may be caused by a cracking or slipping of the fog lamp switch bezel. The bezel may not be able to withstand the driver's force to turn the switch to the 'off' or 'on' positions.

#### CORRECTION:

---------- The condition has been corrected in production. For vehicles exhibiting the condition, new bezels should be used. They are identified as having four ribs on the outside surface of the bezel. Part numbers remain unchanged. (See bezel sketch)

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.