DOES NOT MEET STATE EMISSION INSPECTION - PROCEDURE. Pontiac 6000 1984

For 1990-2009 cars

# DOES NOT MEET STATE EMISSION INSPECTION - PROCEDURE

1984 FIERO, 6000, FIREBIRDS, AND PHOENIX MODELS WITH LR8/LQ9 2.5L ENGINES (VIN CODES R, 2) AND MANUAL TRANSMISSIONS

"Please discard bulletin 84-6(Gasoline)-32, dated 4/86."

If any 1984 Fiero, 6000, Firebird, or Phoenix model with 2.5L engine and manual transmissions experience difficultv meeting the idle exhaust emissions hydrocarbon requirements of state inspection maintenance test programs, and published service manual procedures do not correct the problem, the following list of service PROMS are available from WDDGM:

Service PROM Model Engine Transmission Axle ---- ----- ------ ------------ ---- 1227882 Phoenix 2.5L (LR8) 4-Spd. Manual (M19) 3.65 (GY5)

1227883 Firebird 2.5L (LQ9) 4-Spd. Manual (MO8)

1227884 Firebird 2.5L (LQ9) 5-Spd. Manual (ML3)

1227885 Phoenix 2.5L (LR8) 4-Spd. Manual (MY8) 3.32 (F-25)

1227736 Fiero 2.5L (LR8) 4-Spd. Manual (M19)

Use applicable labor time and operation numbers.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.