RATTLE IN REAR SUSPENSION AREA ANT. CABLE CONTACT WHEELHOUSE. Pontiac 6000 1984

For 1990-2009 cars

# RATTLE IN REAR SUSPENSION AREA ANT. CABLE CONTACT WHEELHOUSE

1984 6000 VEHICLES

A rattle condition may be experienced from the right rear suspension area on some 6000 vehicles equipped with the optional rear mounted power antenna. This condition may be caused by the antenna cable metal connector contacting the top of the right rear inner wheelhouse weld flange.

To eliminate the rattle, use clip 4614452 to attach cable to wheel-house flange as illustrated.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.