CAMSHAFT LOBE LIFT SPECIFICATIONS (CORRECTION). Pontiac 6000 1986

For 1990-2009 cars

# CAMSHAFT LOBE LIFT SPECIFICATIONS (CORRECTION)

CAMSHAFT LOBE LIFT

#### Models Affected: 1985 THROUGH 1988 2.5L ENGINE ----------------- SPECIFICATIONS FOR 6000, GRAND AM AND FIERO MODELS This bulletin is being revised to correct the metric conversion for the camshaft lobe lift.

#### SERVICE MANUAL UPDATE

In the engine specifications charts near the end of the 2.5L engine section, change Camshaft Lobe Lift to:

.232 inches, 5.8928 mm

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.