STALLS ROUGH IDLE DIESEL IDLE ADJUST INFORMATION. Pontiac 6000 1982

For 1990-2009 cars

# STALLS ROUGH IDLE DIESEL IDLE ADJUST INFORMATION

IF EQUIPPED WITH CRUISE CONTROL, IT IS NECESSARY TO DISCONNECT THE CABLE AT THE SERVO ASSEMBLY BEFORE SETTING LOW IDLE SPEED. IF THE CABLE IS ADJUSTED TO MINIMUM SLACK, THE CABLE WILL HOLD THE THROTTLE OFF THE IDLE STOP THEREBY PREVENTING ADJUSTMENT. AFTER SETTING IDLE, RECONNECT THE CABLE TO THE SERVO SELECTING THE HOLE FOR MINIMUM CABLE SLACK.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.