HARSH 1-2 SHIFT 125C TRANSMISSION. Pontiac 6000 1983

For 1990-2009 cars

# HARSH 1-2 SHIFT 125C TRANSMISSION

SOME 1983 THM 125C TRANSMISSION, CC MODEL ONLY, MAY EXHIBIT HARSH 1-2 SHIFTS. BEGINNING AUGUST 5, 1983 ALL CC MODEL THM 125C TRANSMISSIONS WERE PRODUCED WITH A NEW CONTROL VALVE ASSEMBLY THAT HAS A NEW 1-2 ACCUMULATOR VALVE, SPRING AND BUSHING. THE NEW 1-2 ACCUMULATOR VALVE, SPRING AND BUSHING WILL SOFTEN THE 1-2 SHIFT. WHEN SERVICING ANY 1983 CC MODEL THM 125C TRANSMISSION FOR A HARSH 1-2 SHIFT CONDITION, ORDER SERVICE PACKAGE NUMBER 8653944 WHICH CONTAINS: 1 - VALVE, 1-2 ACCUMULATOR 1 - SPRING, 1-2 ACCUMULATOR VALVE 1 - BUSHING, 1-2 ACCUMULATOR VALVE REFER TO YOUR SERVICE MANUAL FOR THE PROPER DISASSEMBLY AND REASSEMBLY OF THE 1-2 ACCUMULATOR VALVE TRAIN.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.