WIRING HARNESS ASSEMBLY USAGE. Pontiac 6000 1989

For 1990-2009 cars

# WIRING HARNESS ASSEMBLY USAGE

#### Models Affected: 1988-90 PONTIAC 6000 STE AND S/E EQUIPPED WITH ALL WHEEL DRIVE AND HYDRA-MATIC 3T40-A

#### BULLETIN COVERS:

Service part information regarding on-vehicle replacement of the torque converter clutch solenoid and wiring harness assembly (333).

#### SERVICE PARTS INFORMATION:

Whenever replacement of the solenoid and wiring harness assembly is necessary, refer to the following part numbers, vehicle model year and transmission identification nameplate.

Use part number 8665356 when:

- the transmission is a 8PBS or 9PBS - the vehicle is a 1988 or 1989 model - a 1990 model service unit is used in a 1988 or 1989 vehicle

Use part number 8665465 when:

- the transmission and vehicle were built in model year 1990

Parts are currently available from GMSPO.

#### SERVICE MANUAL REFERENCE:

Refer to the On-Vehicle Service Section 7A1 of your Pontiac All Wheel Drive Service Manual whenever any on-vehicle service is necessary.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.