HOOD INSULATION MAT DAMAGED. Pontiac 6000 1988

For 1990-2009 cars

# HOOD INSULATION MAT DAMAGED

HOOD INSULATION MAT DAMAGED

#### Models Affected: 1988 6000 ---------------

Customers may comment about damaged in on mat alternator pulley location. This concern can be resolved by cutting 3" x 5" portion of the insulation at the alternator location.

1. Remove fasteners and bend in half the portion of the damaged insulation mat.

2. Cut out 3" x 5" damaged portion of the insulation mat. Care must be taken, not to cut into the hood paint.

3. Reinstall mat with fasteners.

#### Warranty Information

Labor Operation: B1530

Labor Time : .3 Hours

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.