HOIST AND JACKING POINTS COMPONENT PROPER LIFTING. Pontiac Fiero 1984

For 1990-2009 cars

# HOIST AND JACKING POINTS COMPONENT PROPER LIFTING

#### VEHICLES AFFECTED: 1984 Fiero

Please refer to the Fiero Service Manual, page OB-7, for the correct lifting and lacking points on the Fiero.

The locations indicated in the illustration are the only approved lifting and jacking points for the Fiero. Lifting or jacking the car at any other than the designated lifting points could cause damage to underbody mounted components.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.