'DECK AJAR' LIGHT ALWAYS ON INSTALL SWITCH AND P/N'S. Pontiac Fiero 1984

For 1990-2009 cars

# 'DECK AJAR' LIGHT ALWAYS ON INSTALL SWITCH AND P/N'S

1984 FIERO

"Please discard previous bulletin 84-8-23 due to this updated information."

#### CONDITION:

--------- 1. Intermittent or constant "Deck Ajar" light;

2. Rear compartment light always on. (These conditions cause battery drain.)

#### CAUSE:

------ Over-slam of the rear deck lid or misadjustment of the rear compartment light/"Ajar" switch.

#### CORRECTION:

---------- On late production 1984 Fiero models, a white cap switch (Figure 1), is replaced with a black cap switch (Figure 2), Part Number 20545277. All new production Fiero vehicles are equipped with the new black cap switch.

On early production 1984 Fiero models, a black plunger switch (Figure 3), was used. A replacement to this original switch is now available. The replacement switch is Part Number 20629923.

#### CAUTION:

Do not over-torque the nut on either replacement switch.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.