WILL NOT SHIFT OUT OF FIRST GEAR DUE TO THIS DETENT HOLDER. Pontiac Fiero 1986

For 1990-2009 cars

# WILL NOT SHIFT OUT OF FIRST GEAR DUE TO THIS DETENT HOLDER

WILL NOT SHIFT OUT OF FIRST GEAR DUE TO THIN DETENT HOLDER

#### MODELS AFFECTED 1986-1/2 FIERO MODELS WITH 5 SPEED MANUAL --------------- TRANSMISSION (HM-282) AND 2.8L ENGINE

#### BULLETIN COVERS:

Some 1986-1/2 Fiero vehicles equipped with a HM-282 five-speed manual transaxle may have a condition of not being able to shift out of first gear. This is caused by a detent holder that allows the 1-2 shift rail interlock pin to partially come out of the detent holder bore, preventing shifting of the transaxle out of first gear.

To correct this condition, install a thicker detent holder to assure proper retention of the interlock pin.

DATE OF PRODUCTION CHANGE: (Figure 1) -------------------------- Beginning September 8, 1986, all HM-282 transaxles were assembled with the thicker detent holder, thereby eliminating the need for the addition of a spacer plate. Vehicle Identification Number (VIN) break- points are listed below:

Assembly Beginning Up To And Model Plant VIN Including VIN ----- -------- --------- ------------- 1986-1/2 Fiero Pontiac GP200031 GP283971

SERVICE ACTION: (Figure 2) --------------- IMPORTANT: When servicing a 1986 HM-282 built before September 8, 1986, make sure the detent block spacer plate (169 (A)) is reinstalled (if so equipped) during assembly. If there is not a spacer plate, measure the detent holder width. If it is 15mm (0.59 in.) or 16.5mm (0.65 in), replace it with a thicker detent holder, 18mm (0.71 in.) listed under Service Parts Information (Figure 3) .

#### SERVICE MANUAL REFERENCE:

Refer to the appropriate On-Vehicle Service Manual for removal and installation procedures not covered in this bulletin.

#### SERVICE NOTES:

Please record this information in your current service manual for past model service.

#### SERVICE PARTS INFORMATION:

Part Number Description ------ ----------- 08672917 Detent Holder Package - Holder, Detent 18mm (0.71 in.) Thick - Pin, Interlock (Ill. #196) - Pins, Interlock (Ill. #168)

14082039 Cover, Detent Holder

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.