C.E.L. STUMBLE OR NO-START CHECK ENGINE WIRE HARNESS. Pontiac Fiero 1985

For 1990-2009 cars

# C.E.L. STUMBLE OR NO-START CHECK ENGINE WIRE HARNESS

#### VEHICLES AFFECTED: 1985 Fiero With V6 Engines -------------------------- CONDITION: ---------- A wire harness rub-through may cause an intermittent check engine light, engine stumble, no-starts, or an intermittent speedometer.

#### CAUSE:

------ The engine wire harness located over the right hand axle shaft may contact the shaft or axle boot due to excessive slack in the engine wire harness.

#### CORRECTION:

---------- 1. Remove threaded fasteners that hold wire loom harness over axle shaft.

2. Reroute harness by alternator to remove excessive slack (auto trans).

3. For manual trans - eliminate harness droop between fastener clip by having extra length fed toward P.M. generator.

4. Reinstall fasteners.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.