BLOWN GAUGE FUSE-1984 FIERO 20 AMP FUSE REPLACEMENT. Pontiac Fiero 1984

For 1990-2009 cars

# BLOWN GAUGE FUSE-1984 FIERO 20 AMP FUSE REPLACEMENT

#### VEHICLES AFFECTED: 1984 Pontiac Fiero

A condition may occur from repeated deck lid release operation which could cause the 10 amp gauge fuse tu blow. Loss of this circuit will also affect operation of the voltmeter, TCC, cruise control, rear window, defogger, 'Lights On' chime and tachometer.

To repair the above condition, the amperage rating of this fuse has been changed to 20 amps. Sbould you experience a blown gauge fuse and no evidence of a short or ground is apparent, install a 20 amp fuse in the gauge plug of the fuse block.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.