REAR COMPARTMENT TORQUE ROD REPLACEMENT MANUAL. Pontiac Fiero 1985

For 1990-2009 cars

# REAR COMPARTMENT TORQUE ROD REPLACEMENT MANUAL

1984-87 FIERO MODELS

"Please discard bullelin 87-7-28 dated 6/87. This bulletin was published in the wrong section. No other changes were made to the text."

The purpose of this bulletin is to advise of a revision to Figure 7-3, Rear Compartment Torque Rods, shown in Section 7J of all (1984-87) Fiero Service Manuals.

When adjusting or installing torque rod retaininq pins, Item 9, they must be installed from the inboard side as shown in Figure 1.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.