CRUISE CONTROL ACCESSORY KITS INSTALLATION PROCEDURE. Pontiac Fiero 1985

For 1990-2009 cars

# CRUISE CONTROL ACCESSORY KITS INSTALLATION PROCEDURE

1985 FIERO

#### CONDITION:

---------- Cruise Control Accessory kits are incomplete to make a functional cruise system.

#### CAUSE:

------ There are no electrical connections for the servo and vacuum valve on the tail lamp wiring harness unless Option K34 (cruise control) is ordered originally by the dealer.

#### CORRECTION:

----------- * To install a Cruise Control Accessory kit, the tail lamp harness must be replaced with the following assemblies:

1. 2.5 liter engine (L4) - 20481682 2. 2.8 liter engine (V6) - 20603497

* To install either harness requires loosening the roof panel to raise the rear quarter panels. The cruise control wiring is already in the body harness, but it is not in the original rear end harness unless Option K34 was originally ordered.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.