OIL PRESSURE SENSOR SERVICE ADD SHIELD OR RELOCATE SENSOR. Pontiac Fiero 1987

For 1990-2009 cars

# OIL PRESSURE SENSOR SERVICE ADD SHIELD OR RELOCATE SENSOR

#### VEHICLES AFFECTED: 1985-87 FIERO WITH V-6 AND AIR CONDITIONING

Condition: The oil pressure sender on the 1985-1987 Fiero with V-6 engine and air conditioning may become inoperative.

Cause: Water entry into the sender.

Repair: When the sender is replaced, seal the hole in the wire harness connector with filler plug, P/N 12059168, as shown in the Illustration.

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.