Rear Side Door Window Regulator Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the window (8) from the rear side door. Refer to Rear Side Door Window Replacement .
2. Remove the 3 plastic retainers from the regulator electrical connector.
3. Remove the regulator (3) electrical connector from the inner door panel.
4. Disconnect the regulator (3) electrical connector.
5. Remove the 6 regulator mounting screws (1, 3, 4).
6. Slide the regulator through the large opening (2) in the inner door panel.
7. Remove the regulator from the vehicle.

### Installation Procedure

1. Apply a multipurpose grease to all lubrication and sliding points.
2. Install the regulator through the large opening (2) in the inner door panel.
3. Install the regulator to the door. Secure the regulator with the 6 screws (1, 3, 4).

Do not fully tighten the 6 regulator screws (1, 3, 4) at this time.

4. Install the 3 plastic retainers to the electrical connector.
5. Install the regulator electrical connector to the inner door panel.
6. Lower the window to the regulator equalizer bracket. Secure the window with the 2 screws.

Do not tighten the 2 screws at this time.

7. Install the regulator handle.
8. Raise the window completely .
9. Tighten the 6 regulator screws (1, 3, 4).
10. Tighten the 2 window to regulator screws.
11. Remove the regulator handle.
12. Install the rear side door trim panel. Refer to Rear Side Door Window Replacement .