Seat Belt Service Precautions. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Caution: To help avoid personal injury from unrepaired crash damage to a restraint system, perform the seat belt check for each seat belt system. Replace the seat belt system if there is any doubt about the condition of system components.

• | Do not bleach or dye the seat belt webbing. Clean only with a mild soap and water solution and a soft brush or cloth.

• | Keep sharp edges and damaging objects away from the seat belts. Avoid bending or damaging any part of the seat belt buckle or latch plate. Replace any seat belts which are cut or damaged in any way.

• | Use only the correct seat belt anchor bolts/screws and tighten to the correct torque value. Refer to Fastener Tightening Specifications in this section.

| When installing seat belt anchor bolts, start the bolt by hand to ensure that the bolt is threaded straight.

• | Some seat belts and retractors must be serviced as a set with service replacement parts only. Do not attempt to make repairs to the individual components which are only serviced as a set.

• | Verify that the replacement part number is correct for the vehicle at that seating position. Do not substitute a seat belt from a different seating position.