Radio Memory Inoperative. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Radio/Audio System Check

2

1. Disconnect the radio connector.
2. Connect a test lamp from the radio connector cavity 11 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Remove the radio for repair. Is the repair complete? | -- | Go to Radio/Audio System Check | --
4 | Repair the open in the WHT wire between the radio and fuse block 2. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Radio/Audio System Check | --