Blower Motor Always On. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Heater Blower Controls System Check performed? | -- | Go to Step 2 | Go to Heater Blower Controls System Check
2 | Disconnect the blower motor selector switch connector. Does the blower motor stop? | -- | Go to Step 3 | Go to Step 4
3 | Replace the blower speed selector switch. Refer to Blower Switch Replacement . Is the repair complete? | -- | Go to Heater Blower Controls System Check | --
4 | Disconnect the blower motor resistor connector. Does the blower motor stop? | -- | Go to Step 5 | Go to Step 6
5 | Repair the short to voltage in PNK/BLK, PNK/BLU or PNK/GRN wire between the blower speed selector switch and the blower motor resistor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Heater Blower Controls System Check | --
6 | Repair the short to voltage in the PNK wire between the blower speed selector switch, the blower motor resistor and the blower motor. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Heater Blower Controls System Check | --