Windshield Reveal Molding Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Pull the windshield reveal molding (1) away from the windshield (5).
2. Remove the reveal molding (1) from the vehicle.

### Installation Procedure

Important: Trim the reveal molding, as needed, in order to fit the molding in the cavity between the windshield and the windshield pillar.

1. Apply a bead of urethane adhesive from the urethane adhesive kit GM P/N 12346284 into the cavity between the windshield (5) and the windshield pillar.
2. Install the reveal molding (1) to the vehicle.
3. Start from the center of the reveal molding (1) in order to press the reveal molding (1) into place.