Cruise Control Components. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Clutch Pedal Position (CPP) Interrupt Switch (Manual Transmission with Cruise Control) | Under the LH instrument panel mounted to the clutch pedal bracket | Cruise Control Component Views | --
Combination Switch | On the Steering Column | -- | --
Cruise Control Actuator | RH engine compartment near the strut tower | Cruise Control Component Views | --
Cruise Control ON/OFF Switch | LH instrument panel to the right of the steering column | Cruise Control Component Views | --
Cruise Control Mode Switch | RH steering column on the combination switch | -- | --
Fuse Block 1 | RH engine compartment in front of the battery | Power and Grounding Component Views in Wiring Systems | --
C1 (3 Cavities) | Main harness to fuse block 1 below fuse block 1 | Power and Grounding Component Views in Wiring Systems | --
Fuse Block 2 | Under the LH instrument panel | Power and Grounding Component Views in Wiring Systems | --
Instrument Panel Cluster Assembly | LH instrument panel | -- | --
C1 (16 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | Audible Warnings Connector End Views in Instrument Panel, Gauges, and Console
C3 (13 Terminals) | Instrument panel harness to the instrument panel cluster assembly behind the instrument panel cluster assembly | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges, and Console | Audible Warnings Connector End Views in Instrument Panel, Gauges, and Console
Main Relay | Center of the instrument panel behind the blower speed selector | Engine Controls Component Views in Engine Controls - 1.6L | HVAC Connector End Views in HVAC - System
Powertrain Control Module (PCM) | Under the LH instrument panel to the left of the steering column | Engine Controls Component Views in Engine Controls - 1.6L | Powertrain Control Module Connector End Views in Engine Controls - 1.6L
3-Speed Automatic and Manual Transmissions C1 (22 Cavities) | Main harness to the PCM, behind the instrument panel to the left of the steering column | -- | --
Starter Solenoid | Lower RH side of the engine on the starter motor | -- | --
Stoplamp Switch | Under the LH instrument panel above the brake pedal | Lighting Systems Component Views | --
Transmission Range Switch (4-Speed Automatic Transmission) | RH side of the transmission | -- | --
C101 (16 Cavities) | Main harness to the engine harness mounted to the bracket on the bulkhead to the left of the front wiper motor | Harness Routing Views in Wiring Systems | --
C106 (10 Cavities) (4-Speed Automatic Transmission) | Engine harness to the transmission harness, RH rear of the engine under the intake manifold | Harness Routing Views in Wiring Systems | --
C200 (22 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
C201 (16 Cavities) | Main harness to the instrument panel harness, LH instrument panel near fuse block 2 | Harness Routing Views in Wiring Systems | --
G200 | Behind the LH instrument panel above fuse block 2 | Power and Grounding Component Views in Wiring Systems | --
G202 | Behind the center instrument panel on the bulkhead | Power and Grounding Component Views in Wiring Systems | --
P200 | LH rear engine compartment on the bulkhead near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P201 | RH rear engine compartment on the bulkhead near the battery | Harness Routing Views in Wiring Systems | --
S100 (with Cruise) | Main harness approximately 21 cm (8.26 in) from the front wiper motor connector breakout | Harness Routing Views in Wiring Systems | --
S136 | Engine harness approximately 1 cm (0.39 in) from the distributor connector breakout | Harness Routing Views in Wiring Systems | --
S204 | Instrument panel harness approximately at the C211 breakout | Harness Routing Views in Wiring Systems | --
S210 | Main harness approximately 12 cm (4.72 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S214 | Main harness approximately 10 cm (3.93 in) from the C216 breakout | Harness Routing Views in Wiring Systems | --
S215 | Main harness near the powertrain control module (PCM) connector C2 breakout | Harness Routing Views in Wiring Systems | --
S222 | Main harness approximately 10 cm (3.93 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S251 | Main harness approximately 5 cm (1.97 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S252 (with Cruise) | Main harness approximately 5 cm (1.97 in) from the steering column breakout | Harness Routing Views in Wiring Systems | --
S254 | Main harness approximately 10 cm (3.93 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S260 | Main harness approximately 4 cm (1.57 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S262 | Main harness approximately 8 cm (3.15 in) from the stoplamp switch connector breakout | Harness Routing Views in Wiring Systems | --
S264 | Main harness approximately 18 cm (7.09 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S272 | Main harness approximately 11 cm (4.33 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --
S284 | Main harness approximately 7 cm (2.76 in) from the C216 breakout | Harness Routing Views in Wiring Systems | --
S295 | Main harness approximately 7 cm (2.76 in) from the blower speed selector switch connector breakout | Harness Routing Views in Wiring Systems | --
S298 | Main harness approximately 2 cm (0.79 in) from the G200 breakout | Harness Routing Views in Wiring Systems | --