Washer Pump Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Disconnect the front washer pump electrical connector.
2. Disconnect the washer hose (4) from the front washer pump (3).
3. Remove the front washer pump (3) from the washer fluid reservoir (2).

### Installation Procedure

1. Install the front washer pump (3) to the washer fluid reservoir (2).
2. Connect the washer hose (4) to the front washer pump (3).
3. Connect the front washer pump electrical connectors.