Radio Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the heater control knobs from the heater control unit.
2. Remove the heater control unit face plate (2) from the center trim bezel (3) by pulling straight out.
3. Twist off the heater control unit face plate illumination bulb.
4. Remove the ashtray from the track by pushing down on the retainer while pulling the ashtray straight out.
5. Remove the 4 center trim bezel screws (1).
6. Remove the center trim bezel (3).
7. Remove the 4 screws which secure the radio.
8. Remove the radio from the instrument panel by pulling the radio straight out.
9. Disconnect the electrical connector (1) from the radio (3).
10. Disconnect the antenna (2) from the radio (3).
11. Remove the radio from the vehicle.
12. Remove the 4 side mounting bracket screws from the radio (3), as needed.
13. Remove the side mounting brackets.

### Installation Procedure

1. Install the side mounting brackets to the radio (3), if removed. Secure the side mounting brackets with the 4 screws.
2. Connect the antenna (2) to the radio (3).
3. Connect the electrical connector (1) to the radio (3).
4. Install the center trim bezel (3) to the instrument panel. Secure the center trim bezel with the 4 screws (1).
5. Install the ashtray to the track. Push in the ashtray until the retainer engages.
6. Install the heater control unit face plate (2) to the center trim bezel. Push in the heater control unit face plate (2) until the plate snaps into place.
7. Install the heater control knobs to the heater controls.