Fastener Tightening Specifications. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Accelerator Control Cable Adjusting Nut | 25 N·m | 18 lb ft
Accelerator Control Cable Cover Bolts | 15 N·m | 11 lb ft
Air Intake Pipe Bolts | 15 N·m | 11 lb ft
ECT Sensor | 12.5-17.5 N·m | 9.5-12.5 lb ft
EGR Bypass Solenoid Bracket Bolt | 10 N·m | 89 lb in
EGR Pressure Transducer Bracket Bolts | 23 N·m | 17 lb ft
EGR Solenoid Vacuum Valve Bracket Bolts | 10 N·m | 89 lb in
EGR Valve Bolts | 14 N·m | 10.5 lb ft
EVAP Canister Purge Valve Bracket Bolts | 10 N·m | 89 lb in
EVAP Canister Vent Solenoid Bracket Bolt | 10 N·m | 89 lb in
EVAP Tank Pressure Control Solenoid Vacuum Valve Bolt | 10 N·m | 89 lb in
Exhaust Heat Shield Nuts and Bolts | 15 N·m | 11 lb ft
Fuel Pressure Regulator Bolts | 8-12 N·m | 6-8.5 lb ft
Fuel Pulsation Damper | 25-35 N·m | 18.5-25 lb ft
Fuel Rail Bolts | 18-28 N·m | 13.5-20 lb ft
Fuel Rail Plug Bolt | 50 N·m | 36 lb ft
Fuel Filter Mounting Bracket-to-Fuel Filter Bolt | 20 N·m | 15 lb ft
Fuel Filter Mounting Bracket Bolt | 25 N·m | 18 lb ft
Fuel Feed Inlet Hose-to-Fuel Filter Bolt | 35 N·m | 26 lb ft
Fuel Feed Outlet Hose-to-Fuel Filter Bolt | 35 N·m | 26 lb ft
Fuel Feed Outlet Hose-to-Fuel Feed Pipe Bolt | 45 N·m | 33 lb ft
Fuel Filler Pipe Splash Shield Bolts | 15 N·m | 11 lb ft
Fuel Pump-to-Fuel Feed Inlet Hose Bolt | 45 N·m | 33 lb ft
Fuel Tank Pressure Sensor Bolts | 1.2-2.0 N·m | 11-18 lb in
Fuel Tank Protector-to-Fuel Tank Bolt | 25 N·m | 18 lb ft
Fuel Tank Protector and Fuel Tank Mounting Bolts | 35 N·m | 26 lb ft
HO2S 1 | 40-46 N·m | 29-34 lb ft
HO2S 2 | 40-46 N·m | 29-34 lb ft
IAC Valve Bolts | 18-28 N·m | 13.5-20 lb ft
IAT Sensor | 13-17 N·m | 9.5-12 lb ft
MAF Sensor Bolts | 10 N·m | 89 lb in
MAF Sensor Bracket Bolts | 10 N·m | 89 lb in
MAP Sensor Bolts | 10 N·m | 89 lb in
Negative Battery Cable-to-Negative Battery Terminal Retainer Bolt | 15 N·m | 11 lb ft
PCM Support Brace Bolts | 20 N·m | 11 lb ft
PSP Switch | 27 N·m | 20 lb ft
Rear Crossmember Bolts | 70 N·m | 51 lb ft
Throttle Body Bolts | 18-28 N·m | 13.5-20 lb ft
TP Sensor Bolts | 2.5-4.5 N·m | 22.8-38.4 lb in