Rear Door Jamb Switch Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the rubber boot from the rear door jamb switch.
2. Remove the rear body side lower trim panel. Refer to Body Side Rear Trim Panel Replacement in Interior Trim.
3. Disconnect the rear door jamb switch electrical connector.
4. Remove the rear door jamb switch from the vehicle.

### Installation Procedure

1. Connect the rear door jamb switch electrical connector.
2. Install the rear door jamb switch to the door jamb.
3. Install the rubber boot to the rear door jamb switch.
4. Install the rear body side lower trim panel. Refer to Body Side Rear Trim Panel Replacement in Interior Trim.