Rear Side Door Window Switch Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

Notice: The retainer clip must be fully disengaged before the switch plate is removed. Otherwise, damage to the switch plate could result.

1. Gently pry the power window switch from the door trim panel using a taped flat-bladed tool.
2. Disconnect the power window electrical connectors.
3. Remove the power window switch from the vehicle.

### Installation Procedure

1. Connect the power window switch electrical connectors.
2. Install the power window switch by snapping the power window switch into the door trim panel. Ensure that the retaining tabs are fully engaged.