Rear Side Door Window Outer Sealing Strip Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Lower the rear side door window (8) completely.
2. Remove the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .
3. Use a flat-bladed tool wrapped in tape in order to gently pry the outer sealing strip (7) from the door.

### Installation Procedure

1. Install the outer sealing strip (7) to the door by pressing into place.
2. Install the rear side door trim panel. Refer to Rear Side Door Trim Panel Replacement .