Front Side Door Window Belt Inner Sealing Strip Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Use a flat-bladed tool wrapped in tape in order to gently pry the inner sealing strip prongs (2) straight.
3. Remove the inner sealing strip (2) from the door.

### Installation Procedure

1. Install the inner sealing strip (2) to the door by pressing into place. Bend the sealing strip prongs flat in order to secure the strip.
2. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .