Wipers Blades Do Not Park. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Turn ignition to ON.
2. turn the front wiper switch to ON.
3. Turn the front wiper switch to OFF.
4. Backprobe the front wiper motor connector with a J 35616-200 unpowered test lamp from cavity 4 to ground.

Did the test lamp light?

--

Go to Step 3

Go to Step 4

3

1. Manually move the wipers out of the park position.
2. Backprobe the front wiper motor connector with a J 35616-200 unpowered test lamp from cavity 3 to ground.

Did the test lamp light?

--

Go to Step 5

Go to Step 6

4 | Repair the open in the YEL/BLU wire between fuse block 2 and the front wiper motor. Refer to Wiring Repairs in Wiring Systems. Is the repair compete? | -- | Go to Wiper/Washer System Check | --
5 | Replace the front wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Backprobe the front wiper/washer switch connector with a J 35616-200 unpowered test lamp from cavity 14 to ground. Did the test lamp light? | -- | Go to Step 8 | Go to Step 7
7 | Repair the open in the BLU/WHT wire between the front wiper motor and the front wiper/washer switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
8 | Replace the front wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --