Front Seat Recliner Mechanism Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the front seatback cover. Refer to Front Seat Back Cushion Cover Replacement .
2. Remove the recliner mechanism mounting bolt.
3. Remove the recliner mechanism (1) from the seatback.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the recliner mechanism (1) to the front seatback. Secure the recliner mechanism with the mounting bolt.

Tighten
Tighten the front seatback recliner mechanism mounting bolt to 19 N·m (14 lb ft).

2. Install the front seatback cover. Refer to Front Seat Back Cushion Cover Replacement .