Ashtray Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the center trim bezel from the vehicle. Refer to Instrument Panel Center Trim Panel Replacement .
2. Remove the ashtray guide from the instrument panel.
3. Remove the screw and the ashtray illumination lamp, if needed.
4. Twist off the ashtray illumination bulb socket from the lamp, if needed.

### Installation Procedure

1. Install the ashtray illumination bulb socket to the lamp by twisting the socket clockwise, if removed.
2. Install the ashtray illumination lamp to the instrument panel, if removed. Secure the ashtray illuminatation lamp with the screw.
3. Install the ashtray guide to the instrument panel.
4. Install the center trim bezel to the vehicle. Refer to Instrument Panel Center Trim Panel Replacement .