Component Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Lining Thickness (Minimum): 2-Door | 2.5 mm | 0.10 in
Lining Thickness (Minimum): 4-Door | 2.5 mm | 0.10 in
Rotor Lateral Runout (Maximum) | 0.15 mm | 0.006 in
Rotor Surface Finish Depth (Maximum) | 0.38 mm | 0.015 in
Rotor Thickness (Minimum): 2-Door | 8 mm | 0.315 in
Rotor Thickness (Minimum): 4-Door | 15 mm | 0.590 in
Rotor Thickness Variation (Maximum) | 0.013 mm | 0.0005 in