Fastener Tightening Specifications. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Blower Case Retaining Bolts | 10 N·m | 89 lb in
Clutch Coil Wire Retainer Bolt | 2-2.5 N·m | 17.7-22.12 lb in
Compressor Discharge and Suction Hose Bolts | 10 N·m | 8 lb in
Compressor Lower Mounting Bracket Bolts with Power Steering | 18-25 N·m | 13-20 lb ft
Compressor Lower Mounting Bracket Side Bolt without Power Steering | 18-25 N·m | 13-20 lb ft
Compressor Lower Mounting Bracket Bolts without Power Steering | 40-60 N·m | 29-43 lb ft
Compressor Mounting Bolts | 18-28 N·m | 13-20 lb ft
Compressor Upper Bracket Bolts | 40-60 N·m | 29-43 lb ft
Condenser Fan Mounting Bolts | 15 N·m | 11 lb ft
Condenser Inlet Pipe Fitting Bolt | 25 N·m | 18 lb ft
Condenser Mounting Bolts | 20 N·m | 15 lb ft
Condenser Outlet Pipe Fitting Nut | 35 N·m | 26 lb ft
Evaporator Case Mounting Bolts and Nut | 15 N·m | 11 lb ft
Evaporator Inlet Pipe Nut | 35 N·m | 26 lb ft
Evaporator Outlet Pipe Nut | 45 N·m | 33 lb ft
Expansion Valve Pipe (Smaller Nut) | 13 N·m | 115 lb in
Expansion Valve Pipe (Larger Nut) | 35 N·m | 26 lb ft
Front End Upper Panel Bolts | 20 N·m | 15 lb ft
Horn Bolt | 15 N·m | 11 lb ft
Pressure Plate Nut | 15-20 N·m | 10.8-15.2 lb ft
Pressure Relief Valve | 12-18 N·m | 8.7-13 lb ft
Radiator Core Center Brace Bolts | 20 N·m | 15 lb ft
Receiver/Dryer Pipe Fitting Bolt | 35 N·m | 26 lb ft
Refrigerant Pressure Switch | 18 N·m | 13 lb ft