Increase in Effort While Turning Steering Wheel. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Inspect the following components and the following conditions:

• | The joints from the column to the steering gear for wear

• | The joints from the column to the steering gear for proper installation

• | The steering gear valve for the proper installation

• | The power steering pump for the sufficient pressure output

• | The power steering pump for internal leakage

• | The steering gear for internal leakage

• | The power steering hydraulic system

• | The steering gear adjustment

• | The steering gear for binding and rough movement

• | The steering gear mounting for the proper and secure installation

• | The tires for adequate inflation