Rear Door Lock Cylinder Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 14 plastic interior trim panel retaining clips.
2. Remove the rear door interior trim panel (1).
3. Pull the upper portion of the water deflector away from the rear door.
4. Remove the lock cylinder control rod (3) from the lock cylinder (2).
5. Remove the lock cylinder retaining clip (1).
6. Remove the lock cylinder (2) from the rear door.

### Installation Procedure

1. Install the lock cylinder (2) to the rear door. Secure the lock cylinder with the retaining clip (1).
2. Install the lock cylinder control rod (3) to the lock cylinder (2).
3. Inspect the water deflector for tears and holes.
4. Repair the water deflector, as needed, using waterproof tape on either side of the deflector.
5. Apply adhesive to the back of the water deflector.
6. Install the water deflector to the rear door.
7. Install the rear door interior trim panel (1) to the rear door (2). Secure the trim panel with the 14 retaining clips.