Instrument Panel Cluster Trim Plate Bezel Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the 5 screws (2) and the steering column upper and lower covers (1, 3).
2. Remove the 4 screws and the instrument cluster bezel from the vehicle.

### Installation Procedure

1. Install the instrument cluster bezel to the vehicle. Secure the instrument cluster bezel with the 4 screws.
2. Install the steering column upper and lower covers (1, 3). Secure the covers (1, 3) with the 5 screws (2).