Parking Brake Lever Adjustment. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

Important: Ensure the following conditions are met before adjusting the cable:

• | No air is trapped in the brake system, refer to Hydraulic Brake System Bleeding in Brakes

• | Brake pedal travel is within specifications, refer to Brake Pedal Travel in Brakes

• | Brake pedal has been pressed 3 to 10 times with about 30 kg (66 lbs) load

• | Parking brake lever has been pulled up 3 to 10 times with about 20 kg (44 lbs) of pressure and completely released

• | Rear brake shoes are not worn beyond the limit, and the self-adjusting mechanism operates properly

1. Loosen or tighten the locknut (3) until the parking brake is applied with 6 to 8 clicks and 20 kg (44 lbs) of pressure.
2. Secure the locknut after proper adjustment is attained.