Power Window Express Down Function Inoperative. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Power Windows System Check? | -- | Go to Step 2 | Go to Power Windows System Check

2

1. Depress the left front window switch in the left front power window/door lock switch firmly to the DOWN position.
2. Quickly release the switch.

Does the left front window move down automatically to the fully open position?

--

Go to Power Windows System Check

Go to Step 3

3 | Replace the left front power window/door lock switch. Refer to Door Lock and Side Window Switch Replacement . Is the repair complete? | -- | Go to Power Windows System Check | --