Front Bumper Fascia Energy Absorber Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the fascia from the vehicle. Refer to Front Bumper Fascia Replacement .
2. Remove the front bumper energy absorber (2) from the front bumper impact bar (1).

### Installation Procedure

1. Install the front bumper energy absorber (2) to the front bumper impact bar (1).
2. Install the front bumper fascia to the vehicle. Refer to Front Bumper Fascia Replacement .