Front Side Door Window Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

Caution: Wear safety glasses in order to avoid eye damage.

1. Remove the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Lower the front side door window completely.
3. Use a flat-bladed tool wrapped in tape in order to gently pry the inner sealing strip from the door, if equipped.
4. Use a flat-bladed tool wrapped in tape in order to gently pry the outer sealing strip from the door.
5. Remove the screws and the door trim support bracket from the vehicle.
6. Peel the water deflector (1) away from the door.
7. Remove the 2 screws (3) which secure the window (1) to the regulator equalizer bracket (2).
8. Lift the window (1) out from the door.
9. Tilt the top of the window (1) inward in order to clear the regulator run channel.

### Installation Procedure

1. Install the window (1) into the door.
2. Lower the window (1) to the regulator equalizer bracket (2). Secure the window (1) to the bracket (2) with the 2 screws (3).
3. Adjust the regulator equalizer bracket screws so that the measurements between the window and the front side door frame are equal at the points (1, 2).
4. Inspect the water deflector (1) for tears and holes.
5. In order to repair the tears or holes, use waterproof tape on both sides of the water deflector (1), as needed.
6. Apply adhesive (2) to the back of the water deflector (1).
7. Install the water deflector (1) to the door.
8. Install the door trim support bracket to the door. Secure the bracket with the screws.
9. Install the outer sealing strip to the door by pressing into place.
10. Install the inner sealing strip into the door by pressing into place, if equipped.
11. Install the front side door trim panel. Refer to Front Side Door Trim Panel Replacement .