Cigar Lighter Housing Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

The cigar lighter electrical connector and bulb are accessible from behind the left side of the instrument panel.

### Removal Procedure

1. Remove the illumination lamp bulb socket from the cigar lighter.
2. Disconnect the cigar lighter electrical connector.
3. Unscrew the retainer from the rear of the cigar lighter.
4. Remove the cigar lighter from the instrument panel.

### Installation Procedure

1. Install the cigar lighter in the instrument panel. Secure the cigar lighter with the retainer.
2. Connect the electrical connector to the cigar lighter.
3. Install the illumination lamp bulb socket to the cigar lighter.