Daytime Running Lamps (DRL) Resistor Replacement. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the following components from the right front fender:

• | The 2 screws

• | The 6 plastic screws

• | The 1 push clip

• | The wheelhousing

3. Remove the 2 washer fluid reservoir screws.
4. Set aside the washer fluid reservoir.
5. Remove the 2 DRL resistor nuts (2).
6. Reposition the DRL resistor (3).
7. Disconnect the DRL electrical connector (2).
8. Remove the DRL resistor (3) from the vehicle.

### Installation Procedure

1. Connect the DRL resistor electrical connector (2).
2. Install the DRL resistor (3) to the vehicle. Secure the DRL resistor (3) with the 2 nuts.
3. Install the washer fluid reservoir. Secure the washer fluid reservoir with the 2 screws.
4. Install the wheelhouse to the to the right front fender with the following components:

• | The 2 screws

• | The 6 plastic screws

• | The 1 push clip

5. Lower the vehicle.