Strut Assembly Replacement. Pontiac Sun Runner - 2WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Remove the tire and wheel assembly. Refer to Wheel Removal in Tires and Wheels.
3. If the vehicle is equipped with ABS, remove the 1 bolt and the wheel speed sensor harness from the strut.
4. Remove the E-clip that secures the brake hose.
5. Remove the brake hose from the strut.
6. Support the control arm (1) with a floor jack (2).
7. Remove the 2 strut-to-steering knuckle bolts (1) and nuts (3).
8. Remove the strut from the knuckle.
9. Lower the floor jack and the vehicle in order to allow access to the strut upper support nuts.
10. In order to remove the RH front strut upper support nuts, complete the following steps:

10.1. | Remove the 3 bolts for the cruise control bracket (if equipped) and the engine wiring harness bracket.

10.2. | Position the cruise control actuator (if equipped), the engine wiring harness, the brackets, and the fuse block 1 aside in order to access the strut upper support nuts.

11. Remove the 3 strut upper support nuts.
12. Remove the strut from the vehicle.

### Installation Procedure

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

1. Install the strut to the vehicle. Secure the strut with 3 strut support nuts.

Tighten
Tighten the strut upper support nuts to 25 N·m (18 lb ft).

2. If you are installing the RH front strut, secure the engine wiring harness bracket and the cruise control bracket (if equipped) with 3 bolts.

Tighten
Tighten the bracket bolts to 10 N·m (89 lb ft).

3. Raise the vehicle and the floor jack in order to allow access to the steering knuckle.
4. Install the strut to the steering knuckle. Secure the strut with 2 bolts and 2 nuts.

Tighten
Tighten the strut-to-steering knuckle bolts and nuts to 90 N·m (66 lb ft).

5. Remove the floor jack.
6. Install the brake hose to the strut. Secure with an E-clip.
7. If the vehicle is equipped with ABS, install the wheel speed sensor harness to the strut. Secure the harness with the bolt.

Tighten
Tighten the wheel speed sensor harness bolt to 10 N·m (89 lb in).

8. Install the tire and wheel assembly. Refer to Wheel Installation in Tires and Wheels.
9. Lower the vehicle.