Low Oil Pressure Due to Steering Pump. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

Inspect the following components and the following conditions:

• | The flow control valve for the proper operation

• | The pressure plate for the proper mating with the cam ring

• | The cam ring for wear or damage

• | The pressure plate for wear or damage

• | The thrust plate for wear or damage

• | The rotor for wear or damage

• | The rotor slots for the proper vane operation

• | The pump for high internal leakage