Wiper Linkage Replacement - Rear. Pontiac Sun Runner - 4WD (Canada) 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the rear wiper arm. Refer to Rear Window Wiper Arm Replacement .
2. Remove the rear wiper motor. Refer to Rear Window Wiper Motor Replacement .
3. Remove the rear wiper pivot assembly cap (4), the nut, the washer and the gasket from the rear wiper pivot assembly (7).
4. Slide the rear wiper linkage and the rear wiper pivot assembly out of the rear door.
5. Gently pry the rear wiper linkage from the rear wiper pivot assembly.

### Installation Procedure

1. Install the rear wiper linkage to the rear wiper pivot assembly.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Install the rear wiper pivot assembly, with the rear wiper linkage, to the rear door. Secure the rear wiper pivot assembly to the rear door with the gasket, the washer and the nut.

Tighten
Tighten the rear wiper pivot assembly nut to 20 N·m (15 lb ft).

3. Install the rear wiper pivot assembly cap (4) to the pivot assembly (7).
4. Install the rear wiper motor. Refer to Rear Window Wiper Motor Replacement .
5. Install the rear wiper arm. Refer to Rear Window Wiper Motor Replacement .